(kicad_pcb (version 3) (host pcbnew "(2013-mar-13)-testing")
  (general
    (links 62)
    (no_connects 0)
    (area 73.924999 45.924999 119.075001 76.075001)
    (thickness 1.6)
    (drawings 5)
    (tracks 212)
    (zones 0)
    (modules 26)
    (nets 55)
  )
  (page A4)
  (layers
    (15 F.Cu signal hide)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 10)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.8)
    (via_min_drill 0.4)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 74 46)
    (visible_elements FFFFFF1F)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 +3.3V)
  (net 3 /BLUE)
  (net 4 /BOOT0)
  (net 5 /GREEN)
  (net 6 /IR_IN)
  (net 7 /NRST)
  (net 8 /RED)
  (net 9 /SWCLK)
  (net 10 /SWDIO)
  (net 11 /USB_DM)
  (net 12 /USB_DP)
  (net 13 /USB_VBUS)
  (net 14 GND)
  (net 15 N-000001)
  (net 16 N-0000011)
  (net 17 N-0000012)
  (net 18 N-0000015)
  (net 19 N-0000016)
  (net 20 N-0000017)
  (net 21 N-0000018)
  (net 22 N-0000019)
  (net 23 N-0000020)
  (net 24 N-0000021)
  (net 25 N-0000022)
  (net 26 N-0000023)
  (net 27 N-0000024)
  (net 28 N-0000025)
  (net 29 N-0000026)
  (net 30 N-0000027)
  (net 31 N-0000028)
  (net 32 N-0000029)
  (net 33 N-0000030)
  (net 34 N-0000031)
  (net 35 N-0000032)
  (net 36 N-0000033)
  (net 37 N-0000034)
  (net 38 N-0000035)
  (net 39 N-0000036)
  (net 40 N-0000037)
  (net 41 N-0000038)
  (net 42 N-0000039)
  (net 43 N-000004)
  (net 44 N-0000040)
  (net 45 N-0000041)
  (net 46 N-0000042)
  (net 47 N-0000045)
  (net 48 N-0000046)
  (net 49 N-0000047)
  (net 50 N-0000048)
  (net 51 N-000005)
  (net 52 N-0000051)
  (net 53 N-0000052)
  (net 54 N-0000053)
  (net_class Default "Tämä on oletuskytkentäverkkoluokka."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +12V)
    (add_net +3.3V)
    (add_net /BLUE)
    (add_net /BOOT0)
    (add_net /GREEN)
    (add_net /IR_IN)
    (add_net /NRST)
    (add_net /RED)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USB_DM)
    (add_net /USB_DP)
    (add_net /USB_VBUS)
    (add_net GND)
    (add_net N-000001)
    (add_net N-0000011)
    (add_net N-0000012)
    (add_net N-0000015)
    (add_net N-0000016)
    (add_net N-0000017)
    (add_net N-0000018)
    (add_net N-0000019)
    (add_net N-0000020)
    (add_net N-0000021)
    (add_net N-0000022)
    (add_net N-0000023)
    (add_net N-0000024)
    (add_net N-0000025)
    (add_net N-0000026)
    (add_net N-0000027)
    (add_net N-0000028)
    (add_net N-0000029)
    (add_net N-0000030)
    (add_net N-0000031)
    (add_net N-0000032)
    (add_net N-0000033)
    (add_net N-0000034)
    (add_net N-0000035)
    (add_net N-0000036)
    (add_net N-0000037)
    (add_net N-0000038)
    (add_net N-0000039)
    (add_net N-000004)
    (add_net N-0000040)
    (add_net N-0000041)
    (add_net N-0000042)
    (add_net N-0000045)
    (add_net N-0000046)
    (add_net N-0000047)
    (add_net N-0000048)
    (add_net N-000005)
    (add_net N-0000051)
    (add_net N-0000052)
    (add_net N-0000053)
  )
  (module dcsocket-DCSKTN (layer F.Cu) (tedit 522774A0)
    (at 79 58 270)
    (descr "2.1 MM DC SOCKET NEGATIVE PIN")
    (tags "2.1 MM DC SOCKET NEGATIVE PIN")
    (attr virtual)
    (fp_text reference P4 (at 5.36448 3.94462 360) (layer B.SilkS))
    (fp_text value DC21P (at -5.63372 3.30962 360) (layer B.SilkS))
    (pad + thru_hole oval (at 0 -6.07822 270) (size 5.08 2.54) (drill 0.8128)
      (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 1 +12V)
    )
    (pad - thru_hole oval (at 0 -0.07874 270) (size 5.08 2.54) (drill 0.8128)
      (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 14 GND)
    )
    (pad C thru_hole oval (at 4.89966 -3.12928 270) (size 2.54 5.08) (drill 0.8128)
      (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 31 N-0000028)
    )
  )
  (module SM0805 (layer B.Cu) (tedit 5091495C)
    (at 86 51 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10µF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 91.1 65.9)
    (attr smd)
    (fp_text reference C3 (at 0 0) (layer B.SilkS))
    (fp_text value 6.8pF (at 0.09906 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 16 N-0000011)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 93.5 65.9 180)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer B.SilkS))
    (fp_text value 6.8pF (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 17 N-0000012)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 107.1 65.9 90)
    (attr smd)
    (fp_text reference C5 (at 0 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 105.8 59 135)
    (attr smd)
    (fp_text reference C6 (at 0 0 135) (layer B.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 97.6 58.9 45)
    (attr smd)
    (fp_text reference C7 (at 0 0 45) (layer B.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer B.Cu) (tedit 516FD0AE)
    (at 97.6 67.2 315)
    (attr smd)
    (fp_text reference C8 (at 0 0 315) (layer B.SilkS))
    (fp_text value 100nF (at 0.09906 0 315) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_MINI_B (layer B.Cu) (tedit 52282B48)
    (at 77.3 70.25)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB, Mini-B, connector")
    (fp_text reference CON1 (at 0 -6.90118) (layer B.SilkS))
    (fp_text value USB-MINI-B (at 0 7.0993) (layer B.SilkS) hide)
    (pad 1 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038)
      (layers B.Cu B.Paste B.Mask)
      (net 54 N-0000053)
    )
    (pad 2 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038)
      (layers B.Cu B.Paste B.Mask)
      (net 53 N-0000052)
    )
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038)
      (layers B.Cu B.Paste B.Mask)
      (net 52 N-0000051)
    )
    (pad 4 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038)
      (layers B.Cu B.Paste B.Mask)
      (net 36 N-0000033)
    )
    (pad 5 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898)
      (layers B.Cu B.Paste B.Mask)
      (net 35 N-0000032)
    )
    (pad 7 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898)
      (layers B.Cu B.Paste B.Mask)
      (net 34 N-0000031)
    )
    (pad 8 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898)
      (layers B.Cu B.Paste B.Mask)
      (net 33 N-0000030)
    )
    (pad 9 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898)
      (layers B.Cu B.Paste B.Mask)
      (net 32 N-0000029)
    )
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask B.SilkS)
    )
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask B.SilkS)
    )
  )
  (module lm2937-SOT223 (layer B.Cu) (tedit 52277F55)
    (at 80 50 270)
    (descr SOT-223)
    (tags SOT-223)
    (attr smd)
    (fp_text reference IC1 (at 2.3114 2.9464 270) (layer F.SilkS))
    (fp_text value LM2937IMP-3.3 (at 0.635 0.6858 270) (layer F.SilkS))
    (fp_text user >VALUE (at 1.27 0.6858 270) (layer F.SilkS))
    (pad GND smd rect (at 0 -3.0988 270) (size 1.21666 2.23266)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad GND smd rect (at 0 3.0988 270) (size 3.59918 2.19964)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad IN smd rect (at -2.30886 -3.0988 270) (size 1.21666 2.23266)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +12V)
    )
    (pad OUT smd rect (at 2.30886 -3.0988 270) (size 1.21666 2.23266)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
  )
  (module PIN_ARRAY_4x1 (layer F.Cu) (tedit 522830EB)
    (at 115 54.7 270)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value LED_STRIP (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V)
    )
    (pad 2 thru_hole circle (at -1.27 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 51 N-000005)
    )
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 43 N-000004)
    )
    (pad 4 thru_hole circle (at 3.81 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 N-000001)
    )
    (model pin_array\pins_array_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_3X1 (layer F.Cu) (tedit 522830CB)
    (at 115 67.1 270)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0.254 -2.159 270) (layer F.SilkS))
    (fp_text value IR (at 0 -2.159 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 2 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 GND)
    )
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /IR_IN)
    )
    (model pin_array/pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer B.Cu) (tedit 50911E03)
    (at 111.8 52.4 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 2.159 270) (layer B.SilkS))
    (fp_text value IRLML6344 (at 0 0 270) (layer B.SilkS))
    (pad S smd rect (at -0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad G smd rect (at 0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /RED)
    )
    (pad D smd rect (at 0 -1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 51 N-000005)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer B.Cu) (tedit 50911E03)
    (at 111.8 56 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at 0 2.159 270) (layer B.SilkS))
    (fp_text value IRLML6344 (at 0 0 270) (layer B.SilkS))
    (pad S smd rect (at -0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad G smd rect (at 0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /GREEN)
    )
    (pad D smd rect (at 0 -1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 43 N-000004)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer B.Cu) (tedit 50911E03)
    (at 111.8 59.6 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q3 (at 0 2.159 270) (layer B.SilkS))
    (fp_text value IRLML6344 (at 0 0 270) (layer B.SilkS))
    (pad S smd rect (at -0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad G smd rect (at 0.889 1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /BLUE)
    )
    (pad D smd rect (at 0 -1.016 270) (size 0.9144 0.9144)
      (layers B.Cu B.Paste B.Mask)
      (net 15 N-000001)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 99 71.5 270)
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /NRST)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 100.2 68.6 180)
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /BOOT0)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 84.6 68.7 180)
    (attr smd)
    (fp_text reference R3 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 13 /USB_VBUS)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 84.6 67.5 180)
    (attr smd)
    (fp_text reference R4 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 13 /USB_VBUS)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 54 N-0000053)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 84.6 71.1 180)
    (attr smd)
    (fp_text reference R5 (at 0 0 180) (layer B.SilkS))
    (fp_text value 27R (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 11 /USB_DM)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 53 N-0000052)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 5141C458)
    (at 84.6 69.9 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer B.SilkS))
    (fp_text value 27R (at 0.09906 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /USB_DP)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 52 N-0000051)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module LQFP48 (layer B.Cu) (tedit 4C433D64)
    (at 101.7 63.1)
    (attr smd)
    (fp_text reference U1 (at 0 0.381) (layer Cmts.User))
    (fp_text value STM32L151C8 (at 0 -0.381) (layer Cmts.User) hide)
    (pad 12 smd rect (at -4.09702 -2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 46 N-0000042)
    )
    (pad 11 smd rect (at -4.09702 -2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 21 N-0000018)
    )
    (pad 10 smd rect (at -4.09702 -1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 13 /USB_VBUS)
    )
    (pad 9 smd rect (at -4.09702 -1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 8 smd rect (at -4.09702 -0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad 7 smd rect (at -4.09702 -0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /NRST)
    )
    (pad 6 smd rect (at -4.09702 0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 49 N-0000047)
    )
    (pad 5 smd rect (at -4.09702 0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 50 N-0000048)
    )
    (pad 4 smd rect (at -4.09702 1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 17 N-0000012)
    )
    (pad 3 smd rect (at -4.09702 1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 16 N-0000011)
    )
    (pad 2 smd rect (at -4.09702 2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 48 N-0000046)
    )
    (pad 1 smd rect (at -4.09702 2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 48 smd rect (at -2.74828 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 47 smd rect (at -2.2479 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad 46 smd rect (at -1.74752 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 22 N-0000019)
    )
    (pad 45 smd rect (at -1.24714 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 23 N-0000020)
    )
    (pad 44 smd rect (at -0.7493 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /BOOT0)
    )
    (pad 43 smd rect (at -0.24892 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 24 N-0000021)
    )
    (pad 42 smd rect (at 0.24892 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 25 N-0000022)
    )
    (pad 41 smd rect (at 0.7493 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 26 N-0000023)
    )
    (pad 40 smd rect (at 1.24714 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 27 N-0000024)
    )
    (pad 39 smd rect (at 1.74752 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 28 N-0000025)
    )
    (pad 38 smd rect (at 2.2479 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /IR_IN)
    )
    (pad 37 smd rect (at 2.74828 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 9 /SWCLK)
    )
    (pad 25 smd rect (at 4.09702 -2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /RED)
    )
    (pad 26 smd rect (at 4.09702 -2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /GREEN)
    )
    (pad 27 smd rect (at 4.09702 -1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 19 N-0000016)
    )
    (pad 28 smd rect (at 4.09702 -1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /BLUE)
    )
    (pad 29 smd rect (at 4.09702 -0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 39 N-0000036)
    )
    (pad 30 smd rect (at 4.09702 -0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 38 N-0000035)
    )
    (pad 31 smd rect (at 4.09702 0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 30 N-0000027)
    )
    (pad 32 smd rect (at 4.09702 0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 11 /USB_DM)
    )
    (pad 33 smd rect (at 4.09702 1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /USB_DP)
    )
    (pad 34 smd rect (at 4.09702 1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 10 /SWDIO)
    )
    (pad 35 smd rect (at 4.09702 2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad 36 smd rect (at 4.09702 2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
    (pad 13 smd rect (at -2.74828 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 45 N-0000041)
    )
    (pad 14 smd rect (at -2.2479 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 44 N-0000040)
    )
    (pad 15 smd rect (at -1.74752 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 42 N-0000039)
    )
    (pad 16 smd rect (at -1.24714 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 41 N-0000038)
    )
    (pad 17 smd rect (at -0.7493 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 40 N-0000037)
    )
    (pad 18 smd rect (at -0.24892 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 47 N-0000045)
    )
    (pad 19 smd rect (at 0.24892 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 37 N-0000034)
    )
    (pad 20 smd rect (at 0.7493 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 29 N-0000026)
    )
    (pad 21 smd rect (at 1.24714 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 18 N-0000015)
    )
    (pad 22 smd rect (at 1.74752 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 20 N-0000017)
    )
    (pad 23 smd rect (at 2.2479 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (pad 24 smd rect (at 2.74828 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V)
    )
  )
  (module ABS25 (layer B.Cu) (tedit 514F4713)
    (at 90.4 65.2 90)
    (fp_text reference X1 (at 9 1.9 360) (layer B.SilkS) hide)
    (fp_text value CRYSTAL (at 5.2 1.8 90) (layer B.SilkS))
    (pad 1 smd rect (at 1.3 0 90) (size 2 2)
      (layers B.Cu B.Paste B.Mask)
      (net 16 N-0000011)
    )
    (pad 2 smd rect (at 1.3 3.8 90) (size 2 2)
      (layers B.Cu B.Paste B.Mask)
      (net 17 N-0000012)
    )
    (pad M1 smd rect (at 6.8 3.8 90) (size 2 2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad M2 smd rect (at 6.8 0 90) (size 2 2)
      (layers B.Cu B.Paste B.Mask)
    )
  )
  (module C2V10 (layer F.Cu) (tedit 41854742)
    (at 91 52 90)
    (descr "Condensateur polarise")
    (tags CP)
    (fp_text reference C1 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 470µF (at 0 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.778 1.778) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V)
    )
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 GND)
    )
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_4x1 (layer F.Cu) (tedit 522830B4)
    (at 104.9 71.6 180)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value DEBUG (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /NRST)
    )
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /SWDIO)
    )
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 GND)
    )
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.8 1.8) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 /SWCLK)
    )
    (model pin_array\pins_array_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer B.Cu) (tedit 5091495C)
    (at 108 50.5 270)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4.7µF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +12V)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers B.Cu B.Paste B.Mask)
      (net 14 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JPA 2013\nLED wakeup\nlight" (at 93.3 68.6) (layer B.Cu))
  (gr_line (start 74 76) (end 74 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 76) (end 74 76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 46) (end 119 76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74 46) (end 119 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 118 52) (xy 117 53) (xy 108 53) (xy 104 57) (xy 89 57)
        (xy 88 58) (xy 88 61) (xy 87 62) (xy 83 62) (xy 82 61)
        (xy 82 55) (xy 83 54) (xy 87 54) (xy 89 52) (xy 92 52)
        (xy 97 47) (xy 118 47)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 92 51) (xy 89 51) (xy 87 53) (xy 83 53) (xy 81 55)
        (xy 81 61) (xy 80 62) (xy 76 62) (xy 75 61) (xy 75 47)
        (xy 82 47) (xy 82 49) (xy 85 49) (xy 86 48) (xy 92 48)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 74 46) (xy 118.9 46) (xy 119 76) (xy 74 76)
      )
    )
  )
)
