(kicad_pcb (version 3) (host pcbnew "(2013-mar-13)-testing")
  (general
    (links 83)
    (no_connects 0)
    (area 147.924999 66.75 184.536044 98.2086)
    (thickness 1.6)
    (drawings 7)
    (tracks 324)
    (zones 0)
    (modules 35)
    (nets 56)
  )
  (page A4)
  (title_block
    (title "Controller for photography spin plate")
    (rev 1)
    (company jpa)
  )
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal hide)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user hide)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.19)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.5)
    (via_min_size 1)
    (via_min_drill 0.5)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF1F)
    (pcbplotparams
      (layerselection 268468224)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +5V)
  (net 3 +BATT)
  (net 4 /MOTOR_PHASE1)
  (net 5 /MOTOR_PHASE2)
  (net 6 /MOTOR_PHASE3)
  (net 7 /NRST)
  (net 8 /SPEEDCTRL)
  (net 9 /SWCLK)
  (net 10 /SWDIO)
  (net 11 /USART1_RX)
  (net 12 /USART1_TX)
  (net 13 /USBDM)
  (net 14 /USBDP)
  (net 15 /VBUS)
  (net 16 GND)
  (net 17 N-0000013)
  (net 18 N-0000018)
  (net 19 N-0000022)
  (net 20 N-0000023)
  (net 21 N-0000024)
  (net 22 N-0000025)
  (net 23 N-0000026)
  (net 24 N-0000027)
  (net 25 N-0000028)
  (net 26 N-0000029)
  (net 27 N-000003)
  (net 28 N-0000030)
  (net 29 N-0000031)
  (net 30 N-0000032)
  (net 31 N-0000033)
  (net 32 N-0000034)
  (net 33 N-0000035)
  (net 34 N-0000036)
  (net 35 N-0000037)
  (net 36 N-0000038)
  (net 37 N-0000039)
  (net 38 N-000004)
  (net 39 N-0000040)
  (net 40 N-0000041)
  (net 41 N-0000042)
  (net 42 N-0000043)
  (net 43 N-0000044)
  (net 44 N-0000045)
  (net 45 N-0000046)
  (net 46 N-0000047)
  (net 47 N-0000048)
  (net 48 N-0000049)
  (net 49 N-000005)
  (net 50 N-0000050)
  (net 51 N-0000051)
  (net 52 N-0000052)
  (net 53 N-0000054)
  (net 54 N-0000055)
  (net 55 N-000008)
  (net_class Default "Tämä on oletuskytkentäverkkoluokka."
    (clearance 0.19)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net +5V)
    (add_net +BATT)
    (add_net /MOTOR_PHASE1)
    (add_net /MOTOR_PHASE2)
    (add_net /MOTOR_PHASE3)
    (add_net /NRST)
    (add_net /SPEEDCTRL)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USART1_RX)
    (add_net /USART1_TX)
    (add_net /USBDM)
    (add_net /USBDP)
    (add_net /VBUS)
    (add_net GND)
    (add_net N-0000013)
    (add_net N-0000018)
    (add_net N-0000022)
    (add_net N-0000023)
    (add_net N-0000024)
    (add_net N-0000025)
    (add_net N-0000026)
    (add_net N-0000027)
    (add_net N-0000028)
    (add_net N-0000029)
    (add_net N-000003)
    (add_net N-0000030)
    (add_net N-0000031)
    (add_net N-0000032)
    (add_net N-0000033)
    (add_net N-0000034)
    (add_net N-0000035)
    (add_net N-0000036)
    (add_net N-0000037)
    (add_net N-0000038)
    (add_net N-0000039)
    (add_net N-000004)
    (add_net N-0000040)
    (add_net N-0000041)
    (add_net N-0000042)
    (add_net N-0000043)
    (add_net N-0000044)
    (add_net N-0000045)
    (add_net N-0000046)
    (add_net N-0000047)
    (add_net N-0000048)
    (add_net N-0000049)
    (add_net N-000005)
    (add_net N-0000050)
    (add_net N-0000051)
    (add_net N-0000052)
    (add_net N-0000054)
    (add_net N-0000055)
    (add_net N-000008)
  )
  (module PIN_ARRAY_3X1 (layer F.Cu) (tedit 51D19A9E)
    (at 153.8 89.6 90)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0.254 -2.159 90) (layer F.SilkS))
    (fp_text value POT (at 0 -2.159 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 2 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 /SPEEDCTRL)
    )
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 GND)
    )
    (model pin_array/pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY-6X1 (layer F.Cu) (tedit 51D19A86)
    (at 167.64 95.25)
    (descr "Connecteur 6 pins")
    (tags "CONN DEV")
    (fp_text reference P4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value DEBUG (at 0 2.159) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -6.35 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /NRST)
    )
    (pad 2 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /SWDIO)
    )
    (pad 3 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 GND)
    )
    (pad 4 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 /SWCLK)
    )
    (pad 5 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 /USART1_TX)
    )
    (pad 6 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 /USART1_RX)
    )
    (model pin_array/pins_array_6x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_2X1 (layer F.Cu) (tedit 51D19A5E)
    (at 175.26 71.12)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0 -1.905) (layer F.SilkS))
    (fp_text value BATTERY (at 0 -1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT)
    )
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 GND)
    )
    (model pin_array/pins_array_2x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_4x1 (layer F.Cu) (tedit 51D19A4C)
    (at 157.48 71.12 180)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P1 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value MOTOR (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 N-0000018)
    )
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 49 N-000005)
    )
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 38 N-000004)
    )
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 27 N-000003)
    )
    (model pin_array\pins_array_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_MINI_B (layer F.Cu) (tedit 51D034DE)
    (at 178.6 87.8 180)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB, Mini-B, connector")
    (fp_text reference CON1 (at 0 6.90118 180) (layer F.SilkS))
    (fp_text value USB-MINI-B (at 0 -7.0993 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 3.44932 -1.6002 180) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +5V)
    )
    (pad 2 smd rect (at 3.44932 -0.8001 180) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 20 N-0000023)
    )
    (pad 3 smd rect (at 3.44932 0 180) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 26 N-0000029)
    )
    (pad 4 smd rect (at 3.44932 0.8001 180) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 25 N-0000028)
    )
    (pad 5 smd rect (at 3.44932 1.6002 180) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 6 smd rect (at 3.35026 -4.45008 180) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 24 N-0000027)
    )
    (pad 7 smd rect (at -2.14884 -4.45008 180) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 23 N-0000026)
    )
    (pad 8 smd rect (at 3.35026 4.45008 180) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 22 N-0000025)
    )
    (pad 9 smd rect (at -2.14884 4.45008 180) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 21 N-0000024)
    )
    (pad "" np_thru_hole circle (at 0.8509 -2.19964 180) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" np_thru_hole circle (at 0.8509 2.19964 180) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module c_tant_D (layer F.Cu) (tedit 4D5D91AD)
    (at 165.7 77.1 90)
    (descr "SMT capacitor, tantalum size D")
    (fp_text reference C1 (at 0 -2.7305 90) (layer F.SilkS))
    (fp_text value 100µF (at 0 2.7305 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.99974 0 90) (size 2.55016 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 18 N-0000018)
    )
    (pad 2 smd rect (at -2.99974 0 90) (size 2.55016 3.79984)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5091495C)
    (at 178 80.4 180)
    (attr smd)
    (fp_text reference C2 (at 0 -0.3175 180) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +5V)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer F.Cu) (tedit 516FD0AE)
    (at 157.6 83.4 45)
    (attr smd)
    (fp_text reference C3 (at 0 0 45) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer F.Cu) (tedit 516FD0AE)
    (at 164.3 92.9 180)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer F.Cu) (tedit 516FD0AE)
    (at 157.6 91.8 135)
    (attr smd)
    (fp_text reference C5 (at 0 0 135) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer F.Cu) (tedit 516FD0AE)
    (at 166.7 83.5 270)
    (attr smd)
    (fp_text reference C6 (at 0 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_c (layer F.Cu) (tedit 516FD0AE)
    (at 156.2 90.1 270)
    (attr smd)
    (fp_text reference C7 (at 0 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /SPEEDCTRL)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/C0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 49DC4C0B)
    (at 182.2 73.1 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.27 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 19 N-0000022)
    )
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 49DC4C0B)
    (at 182.2 78 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.27 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000052)
    )
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000054)
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 4ECF78EF)
    (at 178 77.6 270)
    (attr smd)
    (fp_text reference IC1 (at 2.19964 -0.29972 360) (layer F.SilkS))
    (fp_text value MCP73831 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000054)
    )
    (pad 3 smd rect (at 0.9525 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT)
    )
    (pad 5 smd rect (at -0.9525 -1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000055)
    )
    (pad 2 smd rect (at 0 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +5V)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer F.Cu) (tedit 50911E03)
    (at 159.56 75.34 180)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value MOSFET_N (at 0 0 180) (layer F.SilkS))
    (pad S smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad G smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /MOTOR_PHASE1)
    )
    (pad D smd rect (at 0 1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 49 N-000005)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer F.Cu) (tedit 50911E03)
    (at 155.96 75.34 180)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value MOSFET_N (at 0 0 180) (layer F.SilkS))
    (pad S smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad G smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /MOTOR_PHASE2)
    )
    (pad D smd rect (at 0 1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 38 N-000004)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer F.Cu) (tedit 50911E03)
    (at 152.36 75.34 180)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q3 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value MOSFET_N (at 0 0 180) (layer F.SilkS))
    (pad S smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad G smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /MOTOR_PHASE3)
    )
    (pad D smd rect (at 0 1.016 180) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 27 N-000003)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 159.56 77.74)
    (attr smd)
    (fp_text reference R2 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /MOTOR_PHASE1)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 155.96 77.74)
    (attr smd)
    (fp_text reference R3 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /MOTOR_PHASE2)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 152.36 77.74)
    (attr smd)
    (fp_text reference R4 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /MOTOR_PHASE3)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 181.2 80.6)
    (attr smd)
    (fp_text reference R5 (at 0 0) (layer F.SilkS))
    (fp_text value 2k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +5V)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000052)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 159.2 80.1 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-000008)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 182.2 70.2 90)
    (attr smd)
    (fp_text reference R7 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 19 N-0000022)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 17 N-0000013)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 156.5 86.1 270)
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /NRST)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 180.6 77 270)
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2k (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000055)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 172.7 88.6)
    (attr smd)
    (fp_text reference R10 (at 0 0) (layer F.SilkS))
    (fp_text value 27R (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /USBDM)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 20 N-0000023)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 172.7 87.5)
    (attr smd)
    (fp_text reference R11 (at 0 0) (layer F.SilkS))
    (fp_text value 27R (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /USBDP)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 26 N-0000029)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module LQFP48 (layer F.Cu) (tedit 4C433D64)
    (at 161.8 87.6)
    (attr smd)
    (fp_text reference U1 (at 0 -0.381) (layer Cmts.User))
    (fp_text value STM32L151C8 (at 0 0.381) (layer Cmts.User) hide)
    (pad 12 smd rect (at -4.09702 2.74828) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 33 N-0000035)
    )
    (pad 11 smd rect (at -4.09702 2.2479) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 35 N-0000037)
    )
    (pad 10 smd rect (at -4.09702 1.74752) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /SPEEDCTRL)
    )
    (pad 9 smd rect (at -4.09702 1.24714) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 8 smd rect (at -4.09702 0.7493) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 7 smd rect (at -4.09702 0.24892) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /NRST)
    )
    (pad 6 smd rect (at -4.09702 -0.24892) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 37 N-0000039)
    )
    (pad 5 smd rect (at -4.09702 -0.7493) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 39 N-0000040)
    )
    (pad 4 smd rect (at -4.09702 -1.24714) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 40 N-0000041)
    )
    (pad 3 smd rect (at -4.09702 -1.74752) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 41 N-0000042)
    )
    (pad 2 smd rect (at -4.09702 -2.2479) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 42 N-0000043)
    )
    (pad 1 smd rect (at -4.09702 -2.74828) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 48 smd rect (at -2.74828 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 47 smd rect (at -2.2479 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 46 smd rect (at -1.74752 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 46 N-0000047)
    )
    (pad 45 smd rect (at -1.24714 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /MOTOR_PHASE3)
    )
    (pad 44 smd rect (at -0.7493 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-000008)
    )
    (pad 43 smd rect (at -0.24892 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /MOTOR_PHASE2)
    )
    (pad 42 smd rect (at 0.24892 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /MOTOR_PHASE1)
    )
    (pad 41 smd rect (at 0.7493 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 17 N-0000013)
    )
    (pad 40 smd rect (at 1.24714 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 36 N-0000038)
    )
    (pad 39 smd rect (at 1.74752 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 28 N-0000030)
    )
    (pad 38 smd rect (at 2.2479 -4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 37 smd rect (at 2.74828 -4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /SWCLK)
    )
    (pad 25 smd rect (at 4.09702 2.74828) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /SWDIO)
    )
    (pad 26 smd rect (at 4.09702 2.2479) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 47 N-0000048)
    )
    (pad 27 smd rect (at 4.09702 1.74752) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 44 N-0000045)
    )
    (pad 28 smd rect (at 4.09702 1.24714) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS)
    )
    (pad 29 smd rect (at 4.09702 0.7493) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 29 N-0000031)
    )
    (pad 30 smd rect (at 4.09702 0.24892) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /USART1_TX)
    )
    (pad 31 smd rect (at 4.09702 -0.24892) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /USART1_RX)
    )
    (pad 32 smd rect (at 4.09702 -0.7493) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /USBDM)
    )
    (pad 33 smd rect (at 4.09702 -1.24714) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /USBDP)
    )
    (pad 34 smd rect (at 4.09702 -1.74752) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /SWDIO)
    )
    (pad 35 smd rect (at 4.09702 -2.2479) (size 0.8001 0.25146)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 36 smd rect (at 4.09702 -2.74828) (size 0.8001 0.24892)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 13 smd rect (at -2.74828 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 51 N-0000051)
    )
    (pad 14 smd rect (at -2.2479 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 50 N-0000050)
    )
    (pad 15 smd rect (at -1.74752 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 43 N-0000044)
    )
    (pad 16 smd rect (at -1.24714 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 48 N-0000049)
    )
    (pad 17 smd rect (at -0.7493 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 45 N-0000046)
    )
    (pad 18 smd rect (at -0.24892 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 31 N-0000033)
    )
    (pad 19 smd rect (at 0.24892 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 30 N-0000032)
    )
    (pad 20 smd rect (at 0.7493 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 21 smd rect (at 1.24714 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 34 N-0000036)
    )
    (pad 22 smd rect (at 1.74752 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 32 N-0000034)
    )
    (pad 23 smd rect (at 2.2479 4.09702) (size 0.25146 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 24 smd rect (at 2.74828 4.09702) (size 0.24892 0.8001)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
  )
  (module c_tant_D (layer F.Cu) (tedit 4D5D91AD)
    (at 170.9 77.1 90)
    (descr "SMT capacitor, tantalum size D")
    (fp_text reference C8 (at 0 -2.7305 90) (layer F.SilkS))
    (fp_text value 100µF (at 0 2.7305 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.99974 0 90) (size 2.55016 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT)
    )
    (pad 2 smd rect (at -2.99974 0 90) (size 2.55016 3.79984)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5091495C)
    (at 168.2 84.2 270)
    (attr smd)
    (fp_text reference C9 (at 0 -0.3175 270) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM2010 (layer F.Cu) (tedit 510157F5)
    (at 168.2 70.7)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference R1 (at 0 -0.7) (layer F.SilkS))
    (fp_text value R (at 0 0.8) (layer F.SilkS))
    (pad 1 smd rect (at -2.4003 0) (size 1.80086 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 18 N-0000018)
    )
    (pad 2 smd rect (at 2.4003 0) (size 1.80086 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT)
    )
    (model smd\chip_smd_pol_wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.35 0.35 0.35))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 167.5 89.2 180)
    (attr smd)
    (fp_text reference R12 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +5V)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 5141C458)
    (at 167.5 90.3)
    (attr smd)
    (fp_text reference R13 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 4ECF78EF)
    (at 171.1 84.3 90)
    (attr smd)
    (fp_text reference U2 (at 2.19964 -0.29972 180) (layer F.SilkS))
    (fp_text value XC6204 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT)
    )
    (pad 3 smd rect (at 0.9525 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT)
    )
    (pad 5 smd rect (at -0.9525 -1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 16 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2013 (at 152.5 84.2) (layer F.Cu))
  (gr_text JPA (at 152.4 81.6) (layer F.Cu))
  (gr_text SPINPLATE (at 156.7 68.6) (layer F.Cu))
  (gr_line (start 148 97) (end 183 97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148 67) (end 148 97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183 67) (end 148 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183 97) (end 183 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill (arc_segments 16) (thermal_gap 0.299999) (thermal_bridge_width 0.299999))
    (polygon
      (pts
        (xy 148 67) (xy 182.9 67) (xy 182.9 96.9) (xy 148 96.9)
      )
    )
  )
)
