(kicad_pcb (version 3) (host pcbnew "(2013-mar-13)-testing")
  (general
    (links 200)
    (no_connects 0)
    (area 212.944445 69.833334 305.075001 120.075001)
    (thickness 1.6)
    (drawings 21)
    (tracks 1251)
    (zones 0)
    (modules 78)
    (nets 70)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.3)
    (via_min_size 0.648)
    (via_min_drill 0.3)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.2)
    (mod_text_size 1 1)
    (mod_text_width 0.2)
    (pad_size 2 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.15)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 215 70)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 15761409)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/petteri/svn-jpa/uunimittari/receiver_pcb/gerber_preview/))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +BATT)
  (net 3 /BOOT0)
  (net 4 /BUTTONS_IN)
  (net 5 /CKV)
  (net 6 /CL)
  (net 7 /D0)
  (net 8 /D1)
  (net 9 /D2)
  (net 10 /D3)
  (net 11 /D4)
  (net 12 /D5)
  (net 13 /D6)
  (net 14 /D7)
  (net 15 "/E Ink Power Supply/+15V")
  (net 16 "/E Ink Power Supply/+22V")
  (net 17 "/E Ink Power Supply/-15V")
  (net 18 "/E Ink Power Supply/-20V")
  (net 19 "/E Ink Power Supply/SHDN_NEG")
  (net 20 "/E Ink Power Supply/SHDN_POS")
  (net 21 /EINK_VDD)
  (net 22 /GMODE)
  (net 23 /LE)
  (net 24 /NRST)
  (net 25 /OE)
  (net 26 /PA6)
  (net 27 /PA7)
  (net 28 /PA8)
  (net 29 "/Power and charge/+5V_IN")
  (net 30 /RL)
  (net 31 /SPEAKER_OUT)
  (net 32 /SPH)
  (net 33 /SPR)
  (net 34 /SPV)
  (net 35 /SWCLK)
  (net 36 /SWDIO)
  (net 37 /USART1_RX)
  (net 38 /USART1_TX)
  (net 39 /USBDM)
  (net 40 /USBDP)
  (net 41 /VBORDER)
  (net 42 /VBORDER_CTRL)
  (net 43 /VCOM)
  (net 44 GND)
  (net 45 N-0000013)
  (net 46 N-0000015)
  (net 47 N-0000017)
  (net 48 N-0000018)
  (net 49 N-0000019)
  (net 50 N-0000022)
  (net 51 N-0000029)
  (net 52 N-0000032)
  (net 53 N-0000055)
  (net 54 N-0000056)
  (net 55 N-0000057)
  (net 56 N-0000058)
  (net 57 N-0000059)
  (net 58 N-0000060)
  (net 59 N-0000065)
  (net 60 N-0000066)
  (net 61 N-0000067)
  (net 62 N-0000068)
  (net 63 N-0000069)
  (net 64 N-000007)
  (net 65 N-0000070)
  (net 66 N-0000071)
  (net 67 N-0000072)
  (net 68 N-0000073)
  (net 69 N-000008)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.3)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net +BATT)
    (add_net /BOOT0)
    (add_net /BUTTONS_IN)
    (add_net /CKV)
    (add_net /CL)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net "/E Ink Power Supply/+15V")
    (add_net "/E Ink Power Supply/+22V")
    (add_net "/E Ink Power Supply/-15V")
    (add_net "/E Ink Power Supply/-20V")
    (add_net "/E Ink Power Supply/SHDN_NEG")
    (add_net "/E Ink Power Supply/SHDN_POS")
    (add_net /EINK_VDD)
    (add_net /GMODE)
    (add_net /LE)
    (add_net /NRST)
    (add_net /OE)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PA8)
    (add_net "/Power and charge/+5V_IN")
    (add_net /RL)
    (add_net /SPEAKER_OUT)
    (add_net /SPH)
    (add_net /SPR)
    (add_net /SPV)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USART1_RX)
    (add_net /USART1_TX)
    (add_net /USBDM)
    (add_net /USBDP)
    (add_net /VBORDER)
    (add_net /VBORDER_CTRL)
    (add_net /VCOM)
    (add_net GND)
    (add_net N-0000013)
    (add_net N-0000015)
    (add_net N-0000017)
    (add_net N-0000018)
    (add_net N-0000019)
    (add_net N-0000022)
    (add_net N-0000029)
    (add_net N-0000032)
    (add_net N-0000055)
    (add_net N-0000056)
    (add_net N-0000057)
    (add_net N-0000058)
    (add_net N-0000059)
    (add_net N-0000060)
    (add_net N-0000065)
    (add_net N-0000066)
    (add_net N-0000067)
    (add_net N-0000068)
    (add_net N-0000069)
    (add_net N-000007)
    (add_net N-0000070)
    (add_net N-0000071)
    (add_net N-0000072)
    (add_net N-0000073)
    (add_net N-000008)
  )
  (module LQFP48 (layer B.Cu) (tedit 515C5D36)
    (at 239.75 94.75)
    (attr smd)
    (fp_text reference U2 (at -0.05 -8.55 180) (layer B.SilkS))
    (fp_text value STM32L151C8 (at -0.05 -7.15 180) (layer B.SilkS))
    (pad 12 smd rect (at -4.09702 -2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 20 "/E Ink Power Supply/SHDN_POS")
    )
    (pad 11 smd rect (at -4.09702 -2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 29 "/Power and charge/+5V_IN")
    )
    (pad 10 smd rect (at -4.09702 -1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 9 smd rect (at -4.09702 -1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 8 smd rect (at -4.09702 -0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 7 smd rect (at -4.09702 -0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 24 /NRST)
    )
    (pad 6 smd rect (at -4.09702 0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 47 N-0000017)
    )
    (pad 5 smd rect (at -4.09702 0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 4 smd rect (at -4.09702 1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 49 N-0000019)
    )
    (pad 3 smd rect (at -4.09702 1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 50 N-0000022)
    )
    (pad 2 smd rect (at -4.09702 2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 22 /GMODE)
    )
    (pad 1 smd rect (at -4.09702 2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 48 smd rect (at -2.74828 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 47 smd rect (at -2.2479 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 46 smd rect (at -1.74752 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /D1)
    )
    (pad 45 smd rect (at -1.24714 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /D0)
    )
    (pad 44 smd rect (at -0.7493 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /BOOT0)
    )
    (pad 43 smd rect (at -0.24892 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 32 /SPH)
    )
    (pad 42 smd rect (at 0.24892 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 33 /SPR)
    )
    (pad 41 smd rect (at 0.7493 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 25 /OE)
    )
    (pad 40 smd rect (at 1.24714 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /LE)
    )
    (pad 39 smd rect (at 1.74752 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /CL)
    )
    (pad 38 smd rect (at 2.2479 4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 21 /EINK_VDD)
    )
    (pad 37 smd rect (at 2.74828 4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 35 /SWCLK)
    )
    (pad 25 smd rect (at 4.09702 -2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 11 /D4)
    )
    (pad 26 smd rect (at 4.09702 -2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /D5)
    )
    (pad 27 smd rect (at 4.09702 -1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 13 /D6)
    )
    (pad 28 smd rect (at 4.09702 -1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 14 /D7)
    )
    (pad 29 smd rect (at 4.09702 -0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 28 /PA8)
    )
    (pad 30 smd rect (at 4.09702 -0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 38 /USART1_TX)
    )
    (pad 31 smd rect (at 4.09702 0.24892) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 37 /USART1_RX)
    )
    (pad 32 smd rect (at 4.09702 0.7493) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 39 /USBDM)
    )
    (pad 33 smd rect (at 4.09702 1.24714) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 40 /USBDP)
    )
    (pad 34 smd rect (at 4.09702 1.74752) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 36 /SWDIO)
    )
    (pad 35 smd rect (at 4.09702 2.2479) (size 0.8001 0.25146)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 36 smd rect (at 4.09702 2.74828) (size 0.8001 0.24892)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 13 smd rect (at -2.74828 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 19 "/E Ink Power Supply/SHDN_NEG")
    )
    (pad 14 smd rect (at -2.2479 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 42 /VBORDER_CTRL)
    )
    (pad 15 smd rect (at -1.74752 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 31 /SPEAKER_OUT)
    )
    (pad 16 smd rect (at -1.24714 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 26 /PA6)
    )
    (pad 17 smd rect (at -0.7493 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 27 /PA7)
    )
    (pad 18 smd rect (at -0.24892 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 30 /RL)
    )
    (pad 19 smd rect (at 0.24892 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 34 /SPV)
    )
    (pad 20 smd rect (at 0.7493 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /CKV)
    )
    (pad 21 smd rect (at 1.24714 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 9 /D2)
    )
    (pad 22 smd rect (at 1.74752 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 10 /D3)
    )
    (pad 23 smd rect (at 2.2479 -4.09702) (size 0.25146 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 24 smd rect (at 2.74828 -4.09702) (size 0.24892 0.8001)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
  )
  (module USB_MINI_B (layer F.Cu) (tedit 515C625E)
    (at 218.8 113.3)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB, Mini-B, connector")
    (fp_text reference P1 (at 5.7 2.9 90) (layer F.SilkS))
    (fp_text value USB-MINI-B (at 0 -7.0993) (layer F.SilkS) hide)
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 29 "/Power and charge/+5V_IN")
    )
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 69 N-000008)
    )
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-000007)
    )
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 7 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 8 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 9 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad "" thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module DFN10 (layer F.Cu) (tedit 515C5C21)
    (at 268.15 86.85 270)
    (attr smd)
    (fp_text reference U3 (at 2.25 2.45 360) (layer F.SilkS))
    (fp_text value LT3463 (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 11 smd rect (at 0 0 270) (size 5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 1 smd rect (at -1 1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 16 "/E Ink Power Supply/+22V")
    )
    (pad 10 smd rect (at -1 -1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000067)
    )
    (pad 2 smd rect (at -0.5 1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 60 N-0000066)
    )
    (pad 9 smd rect (at -0.5 -1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 20 "/E Ink Power Supply/SHDN_POS")
    )
    (pad 3 smd rect (at 0 1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 8 smd rect (at 0 -1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 19 "/E Ink Power Supply/SHDN_NEG")
    )
    (pad 4 smd rect (at 0.5 1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-0000065)
    )
    (pad 7 smd rect (at 0.5 -1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 63 N-0000069)
    )
    (pad 5 smd rect (at 1 1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000070)
    )
    (pad 6 smd rect (at 1 -1.6 270) (size 0.2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 62 N-0000068)
    )
  )
  (module SOT23EBC   placed (layer F.Cu) (tedit 515C5C7F)
    (at 276.6 75 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 2.3 -0.3 180) (layer F.SilkS))
    (fp_text value BC847C (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 45 N-0000013)
    )
    (pad 3 smd rect (at 0 1.016 90) (size 0.9144 0.9144)
      (layers F.Cu F.Paste F.Mask)
      (net 46 N-0000015)
    )
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5   placed (layer F.Cu) (tedit 51742EDE)
    (at 252.5 107.8)
    (attr smd)
    (fp_text reference U5 (at 3 -0.7 180) (layer F.SilkS))
    (fp_text value XC6204 (at 4.9 0.6) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 3 smd rect (at 0.9525 1.27) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 5 smd rect (at -0.9525 -1.27) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0 1.27) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5   placed (layer F.Cu) (tedit 51534F62)
    (at 241.4 114.3 90)
    (attr smd)
    (fp_text reference U4 (at -2.5 0 180) (layer F.SilkS))
    (fp_text value MCP73831 (at -3.9 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000071)
    )
    (pad 3 smd rect (at 0.9525 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 5 smd rect (at -0.9525 -1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 68 N-0000073)
    )
    (pad 2 smd rect (at 0 1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27 90) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 29 "/Power and charge/+5V_IN")
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 51742FED)
    (at 252.5 104.4)
    (attr smd)
    (fp_text reference C14 (at 3.4 0) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 515351A4)
    (at 266.05 91.35 270)
    (attr smd)
    (fp_text reference C5 (at 2.6 1.3 450) (layer F.SilkS))
    (fp_text value 1µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-0000065)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000070)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 516B0338)
    (at 278.45 85.35 270)
    (attr smd)
    (fp_text reference C6 (at -0.05 -1.55 450) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 15 "/E Ink Power Supply/+15V")
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805   placed (layer F.Cu) (tedit 516B03D1)
    (at 266.05 82.25 270)
    (attr smd)
    (fp_text reference C4 (at -2.45 0.45 360) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 516C2285)
    (at 237.3 114.1 270)
    (attr smd)
    (fp_text reference C12 (at 2.5 1.3 540) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 29 "/Power and charge/+5V_IN")
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805   placed (layer F.Cu) (tedit 516B033E)
    (at 278.45 89.65 270)
    (attr smd)
    (fp_text reference C7 (at -0.05 -1.75 450) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516C225E)
    (at 229.3 91.5 270)
    (attr smd)
    (fp_text reference R5 (at -1.9 -0.3 270) (layer F.SilkS))
    (fp_text value 270 (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 48 N-0000018)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 51534EA8)
    (at 273.5 74.1)
    (attr smd)
    (fp_text reference R11 (at -0.1 -1.3) (layer F.SilkS))
    (fp_text value 47k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 31 /SPEAKER_OUT)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 45 N-0000013)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 51535462)
    (at 238.4 100)
    (attr smd)
    (fp_text reference R6 (at 1.8 0.2) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /BOOT0)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 51535477)
    (at 234.3 94 90)
    (attr smd)
    (fp_text reference R7 (at 0 -1.3 90) (layer B.SilkS))
    (fp_text value 10k (at 0.09906 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 24 /NRST)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B03D7)
    (at 270.05 82.45 180)
    (attr smd)
    (fp_text reference R18 (at -0.25 1.95 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 19 "/E Ink Power Supply/SHDN_NEG")
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B036E)
    (at 270.05 90.05)
    (attr smd)
    (fp_text reference R22 (at 0.45 1.25 180) (layer F.SilkS))
    (fp_text value 160k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 62 N-0000068)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 516C2242)
    (at 239.7 111.2)
    (attr smd)
    (fp_text reference R8 (at 1.6 0.4 90) (layer B.SilkS))
    (fp_text value 27 (at 0.09906 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 69 N-000008)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 39 /USBDM)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 516C2240)
    (at 239.7 110.1)
    (attr smd)
    (fp_text reference R9 (at 1.6 -0.3 90) (layer B.SilkS))
    (fp_text value 27 (at 0.09906 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 64 N-000007)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 40 /USBDP)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B0413)
    (at 279.4 75)
    (attr smd)
    (fp_text reference R27 (at 0 1.4) (layer F.SilkS))
    (fp_text value 1k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 46 N-0000015)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B03DE)
    (at 270.05 84.75 180)
    (attr smd)
    (fp_text reference R20 (at -1.65 -0.85 270) (layer F.SilkS))
    (fp_text value 12k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000067)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 51535235)
    (at 266.25 84.75)
    (attr smd)
    (fp_text reference R19 (at -1.1 1.4 90) (layer F.SilkS) hide)
    (fp_text value 200k (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 16 "/E Ink Power Supply/+22V")
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000067)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B03E2)
    (at 270.05 83.55 180)
    (attr smd)
    (fp_text reference R17 (at -1.65 0.75 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 20 "/E Ink Power Supply/SHDN_POS")
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B038E)
    (at 270.05 88.95 180)
    (attr smd)
    (fp_text reference R21 (at -1.65 0.65 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 63 N-0000069)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 62 N-0000068)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516C2256)
    (at 227.1 91.5 270)
    (attr smd)
    (fp_text reference R10 (at -2.4 0.1 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 51534E27)
    (at 218 102 90)
    (attr smd)
    (fp_text reference R15 (at 0.1 -1.4 90) (layer F.SilkS))
    (fp_text value 8.2k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000055)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B0347)
    (at 278.45 92.4 90)
    (attr smd)
    (fp_text reference R23 (at 0 1.75 270) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 51534E67)
    (at 218 94 90)
    (attr smd)
    (fp_text reference R14 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value 3.9k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000056)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 51534E6C)
    (at 218 86 90)
    (attr smd)
    (fp_text reference R13 (at 0.1 -1.4 90) (layer F.SilkS))
    (fp_text value 2k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-0000057)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516C21F0)
    (at 218 78 90)
    (attr smd)
    (fp_text reference R12 (at 0.1 -1.4 90) (layer F.SilkS))
    (fp_text value 1k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000058)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516C2205)
    (at 218 105 270)
    (attr smd)
    (fp_text reference R25 (at 0.1 -2 540) (layer F.SilkS))
    (fp_text value 270 (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 67 N-0000072)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000071)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516AE83B)
    (at 286.9 98)
    (attr smd)
    (fp_text reference R4 (at -2.3 0.1) (layer F.SilkS))
    (fp_text value 47k (at -4.65 0.05) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000059)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516AE838)
    (at 286.9 96.8)
    (attr smd)
    (fp_text reference R2 (at -2.3 -0.1) (layer F.SilkS))
    (fp_text value 100k (at -5.1 -0.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000032)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516AE833)
    (at 286.9 95.6 180)
    (attr smd)
    (fp_text reference R1 (at 2.3 0.2 180) (layer F.SilkS))
    (fp_text value 7.5k (at 4.85 0.2 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000032)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 42 /VBORDER_CTRL)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516AE82E)
    (at 286.9 94.4 180)
    (attr smd)
    (fp_text reference R3 (at 2.3 0.3 180) (layer F.SilkS))
    (fp_text value 100k (at 5.1 0.3 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000032)
    )
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 41 /VBORDER)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516C227C)
    (at 238.9 114.8 90)
    (attr smd)
    (fp_text reference R26 (at -1.8 0 180) (layer F.SilkS))
    (fp_text value 2k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 68 N-0000073)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer B.Cu) (tedit 516C226E)
    (at 234.1 98.8 270)
    (attr smd)
    (fp_text reference C1 (at 1.8 -0.5 450) (layer B.SilkS))
    (fp_text value 7pF (at 0.09906 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 50 N-0000022)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer B.Cu) (tedit 516C226C)
    (at 233 98.8 270)
    (attr smd)
    (fp_text reference C2 (at 1.8 -0.3 450) (layer B.SilkS))
    (fp_text value 7pF (at 0.09906 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 49 N-0000019)
    )
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer F.Cu) (tedit 516C225B)
    (at 228.2 91.5 90)
    (attr smd)
    (fp_text reference C3 (at 1.9 0.1 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /BUTTONS_IN)
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SIL-6 (layer F.Cu) (tedit 51535391)
    (at 241.25 103.85)
    (descr "Connecteur 6 pins")
    (tags "CONN DEV")
    (fp_text reference P3 (at -8.45 0.05 270) (layer F.SilkS))
    (fp_text value DEBUG (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 24 /NRST)
    )
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 36 /SWDIO)
    )
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 35 /SWCLK)
    )
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 38 /USART1_TX)
    )
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 37 /USART1_RX)
    )
  )
  (module SIL-10 (layer F.Cu) (tedit 51535240)
    (at 257.2 71.7)
    (descr "Connecteur 10 pins")
    (tags "CONN DEV")
    (fp_text reference P2 (at 13.7 -0.1 90) (layer F.SilkS))
    (fp_text value EXTENSION (at -4.3 2.1) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT)
    )
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 31 /SPEAKER_OUT)
    )
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 26 /PA6)
    )
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 27 /PA7)
    )
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 /PA8)
    )
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 38 /USART1_TX)
    )
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 51 N-0000029)
    )
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module LED-0805   placed (layer F.Cu) (tedit 515350B2)
    (at 231.1 92.7 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0.1 -1.5 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 47 N-0000017)
    )
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 48 N-0000018)
    )
  )
  (module FH26-39S-0.3SHW (layer B.Cu) (tedit 515350EA)
    (at 288.3 115.4 180)
    (fp_text reference U1 (at 1.95 5.15 180) (layer B.SilkS))
    (fp_text value ED060SC4 (at 7.75 5.15 180) (layer B.SilkS))
    (pad M smd rect (at 0 0.6 180) (size 0.8 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad M smd rect (at 13.2 0.6 180) (size 0.8 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 1 smd rect (at 0.9 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (pad 2 smd rect (at 1.2 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 15 "/E Ink Power Supply/+15V")
    )
    (pad 3 smd rect (at 1.5 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 4 smd rect (at 1.8 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 21 /EINK_VDD)
    )
    (pad 5 smd rect (at 2.1 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /CL)
    )
    (pad 6 smd rect (at 2.4 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /LE)
    )
    (pad 7 smd rect (at 2.7 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 25 /OE)
    )
    (pad 8 smd rect (at 3 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 33 /SPR)
    )
    (pad 9 smd rect (at 3.3 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 10 smd rect (at 3.6 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 11 smd rect (at 3.9 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 32 /SPH)
    )
    (pad 12 smd rect (at 4.2 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /D0)
    )
    (pad 13 smd rect (at 4.5 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /D1)
    )
    (pad 14 smd rect (at 4.8 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 9 /D2)
    )
    (pad 15 smd rect (at 5.1 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 10 /D3)
    )
    (pad 16 smd rect (at 5.4 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 11 /D4)
    )
    (pad 17 smd rect (at 5.7 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /D5)
    )
    (pad 18 smd rect (at 6 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 13 /D6)
    )
    (pad 19 smd rect (at 6.3 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 14 /D7)
    )
    (pad 20 smd rect (at 6.6 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 21 smd rect (at 6.9 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 22 smd rect (at 7.2 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 43 /VCOM)
    )
    (pad 23 smd rect (at 7.5 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 16 "/E Ink Power Supply/+22V")
    )
    (pad 24 smd rect (at 7.8 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (pad 25 smd rect (at 8.1 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 26 smd rect (at 8.4 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
    (pad 27 smd rect (at 8.7 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 22 /GMODE)
    )
    (pad 28 smd rect (at 9 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 22 /GMODE)
    )
    (pad 29 smd rect (at 9.3 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 30 /RL)
    )
    (pad 30 smd rect (at 9.6 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 21 /EINK_VDD)
    )
    (pad 31 smd rect (at 9.9 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (pad 32 smd rect (at 10.2 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 34 /SPV)
    )
    (pad 33 smd rect (at 10.5 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /CKV)
    )
    (pad 34 smd rect (at 10.8 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 41 /VBORDER)
    )
    (pad 35 smd rect (at 11.1 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 21 /EINK_VDD)
    )
    (pad 36 smd rect (at 11.4 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 21 /EINK_VDD)
    )
    (pad 37 smd rect (at 11.7 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 34 /SPV)
    )
    (pad 38 smd rect (at 12 3.4 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /CKV)
    )
    (pad 39 smd rect (at 12.3 0.1 180) (size 0.3 1.2)
      (layers B.Cu B.Paste B.Mask)
    )
  )
  (module SM0402 (layer B.Cu) (tedit 51535458)
    (at 235.7 98.8 315)
    (attr smd)
    (fp_text reference C15 (at 0 0 315) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0.09906 0 315) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer B.Cu) (tedit 51535473)
    (at 235.7 90.7 45)
    (attr smd)
    (fp_text reference C16 (at 0 0 45) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0.09906 0 45) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer B.Cu) (tedit 5153545D)
    (at 243.8 98.8 225)
    (attr smd)
    (fp_text reference C17 (at 0 0 225) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0.09906 0 225) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402 (layer B.Cu) (tedit 5153546F)
    (at 243.8 90.7 315)
    (attr smd)
    (fp_text reference C18 (at 0 0 315) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0.09906 0 315) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 44 GND)
    )
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module ABS25 (layer F.Cu) (tedit 515350DB)
    (at 227.6 94.7 270)
    (fp_text reference X1 (at 9 -1.9 360) (layer F.SilkS))
    (fp_text value 32.768kHz (at 4 2 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.3 0 270) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 50 N-0000022)
    )
    (pad 2 smd rect (at 1.3 -3.8 270) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 49 N-0000019)
    )
    (pad M1 smd rect (at 6.8 -3.8 270) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad M2 smd rect (at 6.8 0 270) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
    )
  )
  (module PIN_ARRAY_2X1 (layer F.Cu) (tedit 51534F13)
    (at 254.7 117.2 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P4 (at 3.4 0 270) (layer F.SilkS))
    (fp_text value BATTERY (at 0 -1.905 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT)
    )
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
    (model pin_array/pins_array_2x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_2X1 (layer F.Cu) (tedit 51534F1F)
    (at 279.9 71.8 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference SP1 (at -3.4 0 270) (layer F.SilkS))
    (fp_text value PIEZO (at 0 -1.905 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT)
    )
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 46 N-0000015)
    )
    (model pin_array/pins_array_2x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 516C21FD)
    (at 216.3 105.6 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D9 (at -1.3 1.8 180) (layer F.SilkS))
    (fp_text value LED (at -0.9 1.6 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 29 "/Power and charge/+5V_IN")
    )
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 67 N-0000072)
    )
  )
  (module sod323 (layer F.Cu) (tedit 51535170)
    (at 267.15 93.85 180)
    (descr SOD323)
    (fp_text reference D2 (at 0 -1.3 180) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 1.19888 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.09982 0 180) (size 1.00076 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000070)
    )
    (pad 1 smd rect (at -1.09982 0 180) (size 1.00076 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (model walter/smd_diode/sod323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module c_tant_D (layer F.Cu) (tedit 51535025)
    (at 254.5 112.9)
    (descr "SMT capacitor, tantalum size D")
    (fp_text reference C13 (at -5.4 0 90) (layer F.SilkS))
    (fp_text value 100µF (at 0 2.7305) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.99974 0) (size 2.55016 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 2 smd rect (at -2.99974 0) (size 2.55016 3.79984)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SELF-WE-TPC_M (layer F.Cu) (tedit 515C5CDA)
    (at 261.7 83.8 180)
    (descr "SELF WE-TPC/M")
    (attr smd)
    (fp_text reference L2 (at 4.1 0 270) (layer F.SilkS))
    (fp_text value 10µH (at 0.8001 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.159 0 180) (size 1.50114 5.30098)
      (layers F.Cu F.Paste F.Mask)
      (net 60 N-0000066)
    )
    (pad 2 smd rect (at 2.159 0 180) (size 1.50114 5.30098)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (model smd/cms_self.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SELF-WE-TPC_M (layer F.Cu) (tedit 515C5CD2)
    (at 261.7 90)
    (descr "SELF WE-TPC/M")
    (attr smd)
    (fp_text reference L1 (at -4.1 0 270) (layer F.SilkS))
    (fp_text value 10µH (at 0.8001 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.159 0) (size 1.50114 5.30098)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT)
    )
    (pad 2 smd rect (at 2.159 0) (size 1.50114 5.30098)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-0000065)
    )
    (model smd/cms_self.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 516B03CB)
    (at 268.15 82.25 270)
    (attr smd)
    (fp_text reference C19 (at -2.45 0.05 540) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 16 "/E Ink Power Supply/+22V")
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 516B03A1)
    (at 268.15 91.35 270)
    (attr smd)
    (fp_text reference C20 (at 1.95 -1.65 270) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HOLE_3MM (layer F.Cu) (tedit 51531F28)
    (at 230 75)
    (fp_text reference HOLE1 (at 0 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module HOLE_3MM (layer F.Cu) (tedit 51531F28)
    (at 230 115)
    (fp_text reference HOLE2 (at 0 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module SM0402_r (layer B.Cu) (tedit 515C5D04)
    (at 258.8 74.1)
    (attr smd)
    (fp_text reference R16 (at 0 1.3) (layer B.SilkS))
    (fp_text value 1k (at 0.09906 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 37 /USART1_RX)
    )
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944)
      (layers B.Cu B.Paste B.Mask)
      (net 51 N-0000029)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module HOLE_3MM (layer F.Cu) (tedit 515C5ED4)
    (at 300 75)
    (fp_text reference HOLE_3MM (at 0 0) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module HOLE_3MM (layer F.Cu) (tedit 515C5EDF)
    (at 300 115)
    (fp_text reference HOLE_3MM (at 0 0) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 515C5BE9)
    (at 289.676 84.605)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value +22V (at 0.124 3.595 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 "/E Ink Power Supply/+22V")
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 515C5BED)
    (at 287.136 84.605)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value +15V (at 0.264 3.595 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 "/E Ink Power Supply/+15V")
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 515C5BF1)
    (at 284.596 84.605)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value -15V (at 0.304 3.595 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 17 "/E Ink Power Supply/-15V")
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 515C5BF6)
    (at 282.056 84.605)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value -20V (at 0.144 3.595 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 "/E Ink Power Supply/-20V")
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 516ACF21)
    (at 292.21 84.6)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value VCOM (at 0.09 3.5 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 43 /VCOM)
    )
  )
  (module SIL-1 (layer F.Cu) (tedit 516ACF2B)
    (at 294.75 84.6)
    (descr "Connecteurs 1 pin")
    (tags "CONN DEV")
    (fp_text reference TP6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value GND (at 0.05 3.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 GND)
    )
  )
  (module SO8E (layer F.Cu) (tedit 516AE827)
    (at 291.45 96.25 270)
    (descr "module CMS SOJ 8 pins etroit")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U6 (at -4.8 0 360) (layer F.SilkS))
    (fp_text value LM358 (at -3.4 0 360) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 15 "/E Ink Power Supply/+15V")
    )
    (pad 1 smd rect (at -1.905 2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 41 /VBORDER)
    )
    (pad 7 smd rect (at -0.635 -2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 43 /VCOM)
    )
    (pad 6 smd rect (at 0.635 -2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 43 /VCOM)
    )
    (pad 5 smd rect (at 1.905 -2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000060)
    )
    (pad 2 smd rect (at -0.635 2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 3 smd rect (at 0.635 2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 52 N-0000032)
    )
    (pad 4 smd rect (at 1.905 2.667 270) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (model smd/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.32 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO8E (layer F.Cu) (tedit 516B0328)
    (at 274.65 83.6)
    (descr "module CMS SOJ 8 pins etroit")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U7 (at 0.05 -4.3) (layer F.SilkS))
    (fp_text value LM78L15ACDG (at 0.25 -5.6) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 16 "/E Ink Power Supply/+22V")
    )
    (pad 1 smd rect (at -1.905 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 15 "/E Ink Power Supply/+15V")
    )
    (pad 7 smd rect (at -0.635 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 6 smd rect (at 0.635 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 5 smd rect (at 1.905 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 2 smd rect (at -0.635 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 3 smd rect (at 0.635 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 4 smd rect (at 1.905 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
    )
    (model smd/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.32 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO8E (layer F.Cu) (tedit 516B031B)
    (at 274.65 91.35)
    (descr "module CMS SOJ 8 pins etroit")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U8 (at 0.25 4.45) (layer F.SilkS))
    (fp_text value LM79L15ACDG (at 0.05 5.85) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 1 smd rect (at -1.905 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 17 "/E Ink Power Supply/-15V")
    )
    (pad 7 smd rect (at -0.635 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (pad 6 smd rect (at 0.635 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (pad 5 smd rect (at 1.905 -2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at -0.635 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (pad 3 smd rect (at 0.635 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
      (net 18 "/E Ink Power Supply/-20V")
    )
    (pad 4 smd rect (at 1.905 2.667) (size 0.59944 1.39954)
      (layers F.Cu F.Paste F.Mask)
    )
    (model smd/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.32 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0402_r (layer F.Cu) (tedit 516B034D)
    (at 278.45 82.55 90)
    (attr smd)
    (fp_text reference R24 (at 0.15 1.55 90) (layer F.SilkS))
    (fp_text value 10k (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 15 "/E Ink Power Supply/+15V")
    )
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (model smd/resistors/R0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module BOURNS_SMD_TRIMMER (layer F.Cu) (tedit 516B0405)
    (at 289.3 99.3 270)
    (fp_text reference RV1 (at 5.4 -2.5 360) (layer F.SilkS))
    (fp_text value 10k (at 2.9 2.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.1 0.5 270) (size 1.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000059)
    )
    (pad 3 smd rect (at 3.4 0.5 270) (size 1.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 44 GND)
    )
    (pad 2 smd rect (at 2.25 -5 270) (size 2 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000060)
    )
  )
  (module B3AL (layer F.Cu) (tedit 516C21EA)
    (at 219 79)
    (fp_text reference SW1 (at -2.3 -5.6 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.85 -7.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000058)
    )
    (pad 2 smd rect (at 6 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
  )
  (module B3AL (layer F.Cu) (tedit 516C21E6)
    (at 219 87)
    (fp_text reference SW2 (at -2.4 -5.4 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.85 -7.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-0000057)
    )
    (pad 2 smd rect (at 6 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
  )
  (module B3AL (layer F.Cu) (tedit 516C21E0)
    (at 219 95)
    (fp_text reference SW3 (at -2.4 -4.8 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.85 -7.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000056)
    )
    (pad 2 smd rect (at 6 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
  )
  (module B3AL (layer F.Cu) (tedit 516C21F8)
    (at 219 103)
    (fp_text reference SW4 (at -2.4 -5.1 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.85 -7.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000055)
    )
    (pad 2 smd rect (at 6 -3.45) (size 2 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
  )
  (gr_text PA5 (at 250.9 74.7 90) (layer F.SilkS))
  (gr_text GND (at 268.7 74.8 90) (layer F.SilkS))
  (gr_text GND (at 266.2 74.8 90) (layer F.SilkS))
  (gr_line (start 305 120) (end 215 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 305 70) (end 305 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215 70) (end 305 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "E Ink display\ncontrol board\n2013 JPA" (at 233.2 81.6) (layer F.SilkS))
  (gr_text RX (at 247.6 106.4 90) (layer F.SilkS))
  (gr_text TX (at 245.1 106.4 90) (layer F.SilkS))
  (gr_text SWCLK (at 242.6 107.9 90) (layer F.SilkS))
  (gr_text GND (at 240 107 90) (layer F.SilkS))
  (gr_text SWDIO (at 237.4 107.8 90) (layer F.SilkS))
  (gr_text NRST (at 234.9 107.3 90) (layer F.SilkS))
  (gr_text +BATT (at 245.8 75.5 90) (layer F.SilkS))
  (gr_text +3.3V (at 248.4 75.4 90) (layer F.SilkS))
  (gr_text PA6 (at 253.4 74.7 90) (layer F.SilkS))
  (gr_text PA7 (at 256 74.6 90) (layer F.SilkS))
  (gr_text PA8 (at 258.4 74.7 90) (layer F.SilkS))
  (gr_text TX (at 261.1 74.3 90) (layer F.SilkS))
  (gr_text RX (at 263.6 74.4 90) (layer F.SilkS))
  (gr_line (start 215 120) (end 215 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 44) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 215 70) (xy 305 70) (xy 305 120) (xy 215 120)
      )
    )
  )
  (zone (net 44) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 215 70) (xy 305 70) (xy 305 120) (xy 215 120)
      )
    )
  )
)
